Nitrogen mass balance of French vertical flow treatment wetlands

Nicolas Forquet

Pascal Molle

Karine Dufossé

Last modified September, 2024

This notebook describes the carbon mass balance estimation for French Vertical Flow (VF) wetlands. It is based on the first LCA inventory carried out by Risch *et al.* (2010). This updated version aims to take better account of experimental data. In particular, it focuses on data collected from a large number of full-scale French VF wetlands.

The mass balance is expressed in .

## Incoming nitrogen flux

Mercoiret *et al.* (2009) estimated the incoming COD flux to 15.5 .

N <- list(inlet = list(total = set\_units(15.5, g/d/pe)))

Mercoiret *et al.* (2009) also provided the ratio of NH4-N/TKN at the inlet of the VF wetland. The average value is 0.74.

Therefore, the mass balance of the inlet can be completed:

bilan.N["water - NH4-N","inlet"] <- N$inlet$total \* 0.74  
bilan.N["water - Norg","inlet"] <- N$inlet$total \* 0.26

## First treatment stage

### Water

The TKN removal rate between the inlet and the outlet of the first treatment stage is obtained from Morvannou *et al.* (2015) : 59%.

The average value of the ratio NH4-N/TKN at the outlet of the first treatment stage has been obtained from an INRAE database and equals 0.79.

TKN.1st.removal <- 0.59  
bilan.N["water - Norg","first.stage"] <- (1-TKN.1st.removal)\*N$inlet$total \* 0.21  
bilan.N["water - NH4-N","first.stage"] <- (1-TKN.1st.removal)\*N$inlet$total \* 0.79

NOx-N are produced by the nitrification of part of the removed TKN. The emission is set to 0.005 . For the first treatment stage, Molle *etl al.* (2008) observed a nitrification rate of 55%.

bilan.N["water - NO2-N","first.stage"] <- 0.005  
bilan.N["water - NO3-N","first.stage"] <- TKN.1st.removal \* N$inlet$total \* 0.55- bilan.N["water - NO2-N","first.stage"]

### Biosolids

Molle (Molle, 2003) measured the N content in the surface deposit of treatment wetland. The estimate is 0.9% of nitrogen in the dry matter.

The biosolids accumulation rate has been estimated in the C mass balance notebook to M.biosolids = 0.02764901 [kg/d/pe].

M.biosolids <- set\_units(0.02764901, kg/d/pe)  
bilan.N["solid - biosolids","first.stage"] <- 0.9/100\*M.biosolids  
print(bilan.N["solid - biosolids","first.stage"])

0.2488411 [g/d/pe]

### Reeds

The nitrogen content in reeds is estimated to 58 by Tanner *et al.* (1996). The surface area of reeds per person is 1.35 . Therefore, the nitrogen content in reeds is 0.21 for the first stage.

bilan.N["solid - reed","first.stage"] <- 58 \* 1.35 / 365.25

### Nitrous oxide emissions

Gaseous emissions on French VF wetlands have been measured by (Filali et al., 2017). For the first stage, gaseous nitrous oxide emissions have been estimated to:

and dissolved nitrous oxide emissions have been estimated to:

bilan.N["gas - N2O-N","first.stage"] <- 0.34/100 \* N$inlet$total  
bilan.N["water - N2O-N","first.stage"] <- 0.25/100 \* N$inlet$total

### N2 emissions

The emissions of have been estimated by difference:

bilan.N["gas - N2-N","first.stage"] <- N$inlet$total - sum(bilan.N$first.stage)

## Second treatment stage

### Water

The TKN removal rate between the inlet and the outlet of the two stages is obtained from Morvannou *et al.* (2015) : 84%.

The average value of the ratio NH4-N/TKN at the outlet of the first treatment stage has been obtained from an INRAE database and equals 0.79.

TKN.overall.removal <- 0.84  
bilan.N["water - Norg","second.stage"] <- (1-TKN.overall.removal)\*N$inlet$total \* 0.21  
bilan.N["water - NH4-N","second.stage"] <- (1-TKN.overall.removal)\*N$inlet$total \* 0.79

The concentration is assumed to be unchanged and equal to 0.005 .

bilan.N["water - NO2-N","second.stage"] <- 0.005

In the PlanteDefi database, the average value of the ratio is 0.477.

bilan.N["water - NO3-N","second.stage"] <- N$inlet$total \* 0.477

### Reeds

The nitrogen content in reeds is estimated to 58 $g N \cdot m^{-2} \cdot y^{-1$ by Tanner *et al.* (1996). The surface area of reeds per person is 0.90 . Therefore, the nitrogen content in reeds is 0.14 for the second stage.

bilan.N["solid - reed","second.stage"] <- 58 \* 0.9 / 365.25

### Nitrous oxide emissions

Gaseous emissions on French VF wetlands have been measured by (Filali et al., 2017). For the first stage, gaseous nitrous oxide emissions have been estimated to:

and dissolved nitrous oxide emissions have been estimated to:

bilan.N["gas - N2O-N","second.stage"] <- 0.43/100 \* N$inlet$total  
bilan.N["water - N2O-N","second.stage"] <- 0.21/100 \* N$inlet$total + bilan.N["water - N2O-N","first.stage"]

Biosolid accumulation at the second stage is negligible and therefore not taken into account.

### N2 emissions

The emissions have been estimated by difference:

bilan.N["gas - N2-N","second.stage"] <- bilan.N["water - Norg","first.stage"] +  
 bilan.N["water - NH4-N","first.stage"] +  
 bilan.N["water - NO3-N","first.stage"] +  
 bilan.N["water - NO2-N","first.stage"] +  
 bilan.N["water - N2O-N","first.stage"] -  
 sum(bilan.N$second.stage)


## Summary

kable(bilan.N)

|  | inlet | first.stage | second.stage |
| --- | --- | --- | --- |
| water - Norg | 4.03 [g/d/pe] | 1.3345500 [g/d/pe] | 0.5208000 [g/d/pe] |
| water - NH4-N | 11.47 [g/d/pe] | 5.0204500 [g/d/pe] | 1.9592000 [g/d/pe] |
| water - NO3-N | 0.00 [g/d/pe] | 5.0247500 [g/d/pe] | 7.3935000 [g/d/pe] |
| water - NO2-N | 0.00 [g/d/pe] | 0.0050000 [g/d/pe] | 0.0050000 [g/d/pe] |
| water - N2O-N | 0.00 [g/d/pe] | 0.0387500 [g/d/pe] | 0.0713000 [g/d/pe] |
| gas - N2O-N | 0.00 [g/d/pe] | 0.0527000 [g/d/pe] | 0.0666500 [g/d/pe] |
| gas - N2-N | 0.00 [g/d/pe] | 3.5605852 [g/d/pe] | 1.2641342 [g/d/pe] |
| solid - biosolids | 0.00 [g/d/pe] | 0.2488411 [g/d/pe] | 0.0000000 [g/d/pe] |
| solid - reed | 0.00 [g/d/pe] | 0.2143737 [g/d/pe] | 0.1429158 [g/d/pe] |

Results can also be presented using a Sankey plot:

Inputs <- as.numeric(c(bilan.N$inlet[1],  
 bilan.N$inlet[2]))  
Inputs <- round(Inputs,2)  
Losses <- as.numeric(c(  
 bilan.N$second.stage[6]+bilan.N$first.stage[6],   
 bilan.N$second.stage[7]+bilan.N$first.stage[7],  
 bilan.N$second.stage[1],  
 bilan.N$second.stage[2],  
 bilan.N$second.stage[4],  
 bilan.N$second.stage[5],  
 bilan.N$first.stage[8],  
 bilan.N$first.stage[9]+bilan.N$second.stage[9],  
 bilan.N$second.stage[3]  
 ))  
Losses <- round(Losses,2)  
Labels <- c("N-org", "NH4-N",  
 "N2O-N", "N2-N",  
 "N-org", "CNH4-N",  
 "NO2-N",  
 "N2O-N", "biosolids-N",  
 "reed", "NO3-N")  
  
  
SankeyR(inputs = Inputs,  
 losses = Losses,  
 unit = "g/d/pe",  
 labels = Labels  
 )



Filali, A., Bollon, J., Molle, P., Mander, Ü., Gillot, S., 2017. High-frequency measurement of N2O emissions from a full-scale vertical subsurface flow constructed wetland. Ecological Engineering 108, 240–248. <https://doi.org/10.1016/j.ecoleng.2017.08.037>

Mercoiret, L., 2009. Qualité des eaux usées domestiques produites par les petites collectivités. ONEMA.

Molle, P., 2003. [Filtres plantés de roseaux : limites hydrauliques et rétention du phosphore](https://hal.inrae.fr/tel-02583262) (PhD thesis).

Molle, P., Prost-Boucle, S., Lienard, A., 2008. Potential for total nitrogen removal by combining vertical flow and horizontal flow constructed wetlands: A full-scale experiment study. Ecological Engineering 34, 23–29. <https://doi.org/10.1016/j.ecoleng.2008.05.016>

Morvannou, A., Forquet, N., Michel, S., Troesch, S., Molle, P., 2015. Treatment performances of French constructed wetlands: Results from a database collected over the last 30 years. Water Science and Technology 71, 1333–1339. <https://doi.org/10.2166/wst.2015.089>

Risch, E., Boutin, C., 2010. Rapports d’ACV et données d’inventaire.

Tanner, C.C., 1996. Plants for constructed wetland treatment systems A comparison of the growth and nutrient uptake of eight emergent species. Ecological Engineering 7, 59–83. <https://doi.org/10.1016/0925-8574(95)00066-6>